REM 1942 Pacific Air War by Mircorprose

REM This file for use with the MARK II Weapons Control System
REM from THRUSTMASTER (A really cool product!)

REM To use this file with your MARK II WCS

REM Set RED switch to DIGITAL
REM Set BLACK switch to ANALOG

REM If the RED switch is set to ANALOG, you will have to choose
REM the THROTTLE WHEEL as the throttle control type

REM if the BLACK swith is set to DIGITAL and your FCS is plugged
REM into your WCS MARK II your HAT will not be as functional as
REM when the BLACK swith is set to ANALOG and you select
REM FCS HAT FROM THRUSTMASTER as your CAMERA DEVICE within 1942

REM ** If your joystick is plugged into the WCS MARK II, you
REM ** should not select JOYSTICK 1 or 2 as your camera device.
REM ** Instead you should use a mouse or the keyboard

GAME 2 100 rem Type 2 throttle, 100ms delay should be alright

BTN UB /U c			 rem Centers the Virtual Cockpit View (except in padlock)
       /M c			 rem Centers the Virtual Cockpit View
       /D /N TAB   rem Fire Rockets (if available)

BTN MB /U ALT e
       /M ALT e
       /D ENT      rem Drop Primary Load (usually bombs)

BTN LB /U ALT e
       /M ALT e
       /D BSP      rem Drop Secondary Load (sometimes fueltanks)

BTN 3  /U ALT e
       /M ALT e
       /D /N TAB      rem Fire Rockets (if available)

BTN 2  /U ALT e
       /M ALT e
       /D /N ENT      rem Drop Primary Load (usually bombs)

BTN 1  /U ALT e
       /M ALT e
       /D /N BSP      rem Drop Secondary Load (sometimes fueltanks)

BTN HU F1          rem Forward View
BTN HR F3          rem Right View
BTN HD /T F4       rem Left Shoulder View Followed by Right Shoulder View
       /T F5
BTN HL F2          rem Left View

BTN 4 /T ALT F1    rem Toggle Virtual Cockpit or Tailgunner view
      /T F1        rem and COCKPIT VIEW

BTN 5 /T F6        rem First press == CHASE VIEW
      /T F1	   rem Second press == COCKPIT VIEW

BTN 6 /U /N g      rem Landing Gear or Bomb Sight view
      /M /N g
      /D ALT F2


BTN MT /P /N _     rem Go to 0 Throttle on back
		 /R 1        rem Start at 1 for forward

THR 8 3 1 2 3 4 5 6 7 8 9 0 +  rem Seven steps ending in + to insure max throttle

rem NOTE: THIS FILE IS TO BE USED WITH THE NEW CHIP AND MICROCODE FOR THE
rem MARK II WCS ONLY.  IF YOU DO NOT HAVE THIS CHIP, THEN CONTACT THRUSTMASTER
rem TO INQUIRE ABOUT UPGRADING TO THE NEW CHIP AND MICROCODE!!!!
rem How can you tell if you have the new chip and microcode?  At the C:\MARK2
rem Dos prompt type DIR MK2LOAD.EXE and hit enter.  If it says "File not found
rem then you have the old microcode version that uses DOWNLOAD.EXE instead.

