64VBE101.ZIP - ATI Technologies Inc.
ллллллллллллллллллллллллллллллллллллллллллллл   ATI Technologies Inc.
лллллллл(R)лллп                      ммм  плл   33 Commerce Valley Drive East
ллллллллллллп                        ппп  млл   Thornhill, ON  L3T 7N6
ллллллллллп      мллллл     ллллллллллллллллл   CANADA
ллллллллп      мллппллл     ллллллллп   плллл
ллллллп      мллл    лл     лллллллл     лллл   Support:     (905) 882-2626
ллллп      мллллллммллл     лллллллл     лллл   Support FAX: (905) 882-0546
ллп      мллллллллллллл     лллллллл     лллл   Compuserve:  GO ATITECH
ллм    млллллллллллллллм   мллллллллм   млллл   кФФФФФФФФФФФФФФФФФФФФФФФФФФФФФП
ллллппппппппппппппппппппппппппппппппппппллллл   Г         ATI mach64          Г
лллн T E C H N O L O G I E S    I N C . олллл   Г VESA BIOS Extension utility Г
ллллммммммммммммммммммммммммммммммммммммллллл   Г        version 1.01         Г
ллллллллллллллллллллллллллллллллллллллллллллл   РФФФФФФФФФФФФФФФФФФФФФФФФФФФФФй

 Length  Method   Size  Ratio   Date    Time    CRC-32  Attr  Name
 ------  ------   ----- -----   ----    ----   -------- ----  ----
   5377  Implode   2298  58%  05-12-95  14:09  9826bf23 --w-  README.VBE
   1448  Implode    895  39%  04-13-95  17:10  9b9a0882 --w-  REPORT.TXT
   5274  Implode   3032  43%  02-21-95  11:18  58d0d2ac --w-  M64VBE.COM
   9297  Implode   6145  34%  04-08-94  16:42  1c815864 --w-  VESATEST.EXE
 ------          ------  ---                                  -------
  21396           12370  43%                                        4

***********************************************************************
mach64 VESA Support
***********************************************************************

READ THIS FILE COMPLETELY BEFORE ATTEMPTING TO USE THIS PRODUCT!

****************************

Contents

1.0     Supported VESA modes
2.0     mach64 VESA TSR 
3.0 	Installation of the BBS version

****************************

1.0     Supported VESA modes

The VESA modes supported by your mach64 card are dependent upon the 
amount of video memory and the monitor type selected in the ADVANCED or 
QUICK SETUP.

In order to determine the actual VESA modes supported by your current 
configuration you should run VESATEST.EXE.  VESATEST is an ATI specific
utility which has been included in 64VBE101.ZIP for your convenience.


****************************

2.0     mach64 VESA TSR 

If you experience any problems with applications that use VESA modes,  
install and run the ATI mach64 Terminate and Stay Resident (TSR) VESA  
program M64VBE.COM. 

The default settings for M64VBE.COM are:

- dual read and write windows enabled
- 320 modes enabled
- VGA Wonder memory paging disabled
- VGA CRT parameters enabled

****************************

3.0 	Installation of the BBS version

To install the BBS version of M64VBE.COM and VESATEST.EXE:

1. Ensure that you have a copy of PKUNZIP.EXE, v1.10 or later.  PKUNZIP
is available on most BBS and information services, including the ATI
BBS and CompuServe.

2. Unzip 64VBE101.ZIP into the mach64 directory on your hard disk. For example:

PKUNZIP 64VBE101.ZIP \MACH64
CD \MACH64

The following files will be copied to the mach64 directory:

README.VBE
REPORT.TXT
M64VBE.COM
VESATEST.EXE

To load the TSR type:     M64VBE <enter> 

To un-install the mach64 VESA TSR Change directory to the c:\mach64 
(default) and type M64VBE U <enter>.

Note: If you experience any problems unloading the TSR please consult 
your DOS documentation for TSR un-install limitations.


To determine the modes supported by your current configuration you must 
run VESATEST from the mach64 directory.  


