REM Pacific Strike by Origin
REM Set BLACK and RED switches to DIGITAL.
REM Select JOYSTICK for stick control. Throttle is keyboard.
      
GAME 2 120       REM Game type 2; 120 ms delay
BTN UB w         REM Weapon select
BTN MB F1        REM Return to front view
BTN LB n         REM Brings up nav map
BTN HU KP8       REM Pan up
BTN HR KP6       REM Pan right
BTN HD KP2       REM pan down
BTN HL KP4       REM Pan left

BTN 1 CTL B      REM Opens the top and jumps out!!!!
BTN 2 F6         REM Cycles Through External views of all planes.
BTN 3 t          REM Target select
BTN 4 CTL t      REM Ground Target Select
BTN 5 f          REM Flaps
BTN 6 b          REM Brakes
RKR UP G         REM Gun Selection
RKR DN G         REM Gun Selection
THR 9 1 1 2 3 4 5 6 7 8 9 0

rem NOTE: THIS FILE IS TO BE USED WITH THE NEW CHIP AND MICROCODE FOR THE
rem MARK II WCS ONLY.  IF YOU DO NOT HAVE THIS CHIP, THEN CONTACT       THRUSTMASTER
rem TO INQUIRE ABOUT UPGRADING TO THE NEW CHIP AND MICROCODE!!!!
rem How can you tell if you have the new chip and microcode?  At the C:\MARK2
rem Dos prompt type DIR MK2LOAD.EXE and hit enter.  If it says "File not found
rem then you have the old microcode version that uses DOWNLOAD.EXE instead.
	
