;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU
;UU                                                                        UU
;UU  Miles Design Audio Interface Library                                  UU
;UU                                                                        UU
;UU  Sound driver installation message file                                UU
;UU                                                                        UU
;UU  Default selection criteria/examples:                                  UU
;UU                                                                        UU
;UU    .E BLASTER ........ Environment var 'BLASTER' must be present       UU
;UU    .C MVSOUND ........ CONFIG.SYS must contain 'MVSOUND' string        UU
;UU    .A AWEUTIL ........ AUTOEXEC.BAT must contain 'AWEUTIL' string      UU
;UU                                                                        UU
;UU    .NE BLASTER ....... Environment var 'BLASTER' must NOT be present   UU
;UU    .NC MVSOUND ....... CONFIG.SYS must NOT contain 'MVSOUND' string    UU
;UU    .NA AWEUTIL ....... AUTOEXEC.BAT must NOT contain 'AWEUTIL' string  UU
;UU    .ND  .............. Entry cannot be selected as default             UU
;UU                                                                        UU
;UU    .T1  .............. Optional BLASTER Tn, if present, must be 1|3    UU
;UU    .T2  .............. Mandatory BLASTER Tn must be 2|4|5              UU
;UU    .T3  .............. Mandatory BLASTER Tn must be >=6                UU
;UU                                                                        UU
;UU  I/O default derivation:                                               UU
;UU                                                                        UU
;UU    .IOB .............. Derive I/O defaults from BLASTER variable       UU
;UU    .IOD .............. I/O defaults = first driver default entry       UU
;UU    .ION .............. Do not allow manual I/O configuration at all    UU
;UU                                                                        UU
;UU    .IOA .............. Use I/O address only (must appear at end)       UU
;UU    .IOL .............. Suppress high-DMA prompt (must appear at end)   UU
;UU                                                                        UU
;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sblaster.dig]

;
;Selected by default if BLASTER variable is of type T1 or T3 (or no T 
;specifier), and no other "clone" variable exists (ULTRASND, MVSOUND, etc.)
;
;Default I/O parms from BLASTER
;

.E BLASTER
.T1
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOL

.SPECIAL_TEXT
Seleziona questo driver per la Sound Blaster, la Sound Galaxy,
la Thunderboard o la Pro Audio Spectrum.  Altre schede potrebbero 
funzionare con questo driver se sono compatibili via hardware con
la Sound Blaster senza bisogno di driver di emulazione o TSR.

.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbpro.dig]

;
;Selected by default if BLASTER variable is of type T2, T4, or T5
;and no other "clone" variable exists
;
;Default I/O parms from BLASTER
;

.E BLASTER
.T2
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOL

.SPECIAL_TEXT
Questo driver gestisce tutte le versioni Sound Blaster Pro e
100% compatibili.  Non Š raccomandato l'uso con la Sound 
Blaster 16 o l'AWE32.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sb16.dig]

;
;Selected by default if BLASTER variable is of type T6
;
;Default I/O parms from BLASTER (I/O address only)
;

.E BLASTER
.T3
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOA

.SPECIAL_TEXT
Per l'audio digitale ad alta qualit… con la Sound Blaster 16 o AWE32 
seleziona questo driver.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[rap10.dig]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.HIGH_DMA_PAIRS

.SPECIAL_TEXT
AVVERTIMENTO: Durante l'autorilevamento della Roland RAP-10, il driver
verifica la presenza della RAP-10 con l'indirizzo I/O di 320H o 330H.  
Non rileva il canale DMA n‚ i settaggi IRQ.  Se la scheda RAP-10 
non Š configurata con IRQ 9 o se i canali DMA 5 e 6 sono impegnati
da un'altra scheda del sistema, dovrai selezionare la 
"Configurazione Manuale" e quindi dovrai inserire i settaggi I/O per la 
tua scheda. Altrimenti, il sistema potrebbe bloccarsi oppure potrebbero 
verificarsi delle interferenze durante il playback.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[proaudio.dig]

;
;Selected by default if CONFIG.SYS contains MVSOUND string
;
;No configuration allowed
;

.C MVSOUND.SYS
.ION

.SPECIAL_TEXT
L'audio digitale stereo Š disponibile, con questo driver, con tutte le 
versioni della Pro Audio Spectrum Mediavision. Se si verificano
dei problemi, dovresti scegliere il driver Sound Blaster-compatibile.
L'utility della Media Vision, MVSOUND.SYS, dovr… essere caricata in 
memoria. Nel caso contrario la scheda non verr… rilevata.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[ultra.dig]

;
;Selected by default if environment contains ULTRASND variable
;
;Default I/O parms from driver
;

.E ULTRASND
.IOD

.SPECIAL_TEXT
Quando utilizzi questo driver, assicurati che non ci siano utility Gravis  
come Sbos, UltraMID o Mega-Em attive. E' meglio disporre della versione 2.0 
del software di sistema Ultrasound.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[jammer.dig]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.NAME
New Media Corporation WaveJammer(TM) Digital Audio

.SPECIAL_TEXT
La scheda WaveJammer della New Media Corporation fornisce un suono di   
altissima qualit… su interfaccia PCMCIA.  Seleziona il driver Ad Lib(R) Music
Synthesizer Card per l'audio FM.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sndscape.dig]

;
;Selected by default if environment contains SNDSCAPE variable
;
;Default I/O parms from driver
;

.E SNDSCAPE
.IOD

.NAME
Ensoniq SoundScape(TM) Digital Audio

.SPECIAL_TEXT
Seleziona questo driver per la scheda Ensoniq SoundScape(TM) o compatibile.

.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sndsys.dig]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.NAME
Microsoft(R) Windows(TM) Sound System oppure compatibile al 100%

.SPECIAL_TEXT
Seleziona questo driver se la tua scheda Š compatibile con Microsoft
Windows Sound System.

Se il canale DMA 1 non Š disponibile per la scheda Windows Sound System, 
dovrai selezionare l'opzione "Configurazione manuale" per selezionare un 
altro canale DMA. Se stai lavorando sotto Windows 95 
o un altro sistema Plug-n-Play, dovrai controllare il Gestore di Periferica 
per verificare quale indirizzo I/O sta utilizzando la scheda Windows Sound
System.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[adrv688.dig]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.NAME
ESS Technology ES688 Digital Audio

.SPECIAL_TEXT
Questo driver gestisce i sistemi dotati del chipset ES688 della ESS
Technology.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[mpu401.mdi]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.SPECIAL_TEXT
La maggior parte dei sintetizzatori General MIDI gestisce l'interfaccia 
MIDI MPU-401. Questi comprendono Roland Sound Canvas, RAP-10, e 
compatibili, oltre alle schede add-on della famiglia Sound Blaster
16. I dispositivi MPU-401 generalmente forniscono un'altissima qualit…     
sonora, ma gli utenti delle periferiche Adaptec SCSI potrebbero decidere  
di utilizzare l'opzione "Configurazione manuale" per ridurre probabili 
problemi di rilevamento con la MPU-401. 
Se possiedi una scheda AWE-32 della Creative Labs, dovresti selezionare 
"Creative Labs AWE-32(TM) General MIDI".
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sndscape.mdi]

;
;Selected by default if environment contains SNDSCAPE variable
;
;Default I/O parms from driver
;

.E SNDSCAPE
.IOD

.NAME
Ensoniq SoundScape(TM) General MIDI

.SPECIAL_TEXT
Seleziona questo driver per la scheda Ensoniq SoundScape(TM) o compatibile.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[ultra.mdi]

;
;Selected by default if environment contains ULTRASND variable
;
;Default I/O parms from driver
;

.E ULTRASND
.IOD

.SPECIAL_TEXT
Quando usi questo driver, Š importante che non ci siano utility della
Gravis come SBOS, UltraMID o Mega-Em attive. E' meglio disporre della 
versione 2.0 o successiva del software di sistema UltraSound.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbawe32.mdi]

;
;Selected by default if AUTOEXEC contains AWEUTIL string
;
;Default I/O parms from driver
;

.A AWEUTIL
.IOD

.NAME
Creative Labs AWE-32(TM) General MIDI

.SPECIAL_TEXT
Questo driver genera un'audio di qualit… General MIDI wavetable con la scheda
Creative Labs AWE-32. Il driver "Creative Labs Sound Blaster 16 o AWE32"
deve essere selezionato per l'audio digitale.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sblaster.mdi]

;
;Selected by default if BLASTER variable is of type T1 or T3 (or no T 
;specifier), and no other "clone" variable exists (ULTRASND, MVSOUND, etc.)
;
;Default I/O parms from BLASTER (A only)
;

.E BLASTER
.T1
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOA

.SPECIAL_TEXT
Questo driver pu• essere utilizzato con tutte le schede Sound Blaster 
compatibili che non ricercano i driver TSR per attivare la compatibilit…
Sound Blaster FM. Gli utenti di schede sonore pi— sofisticate basate su 
General MIDI possono selezionare il driver Sound Blaster solo se 
si verificano problemi col driver General MIDI, siccome il vecchio chipset
OPL-2 Sound Blaster non offre la qualit… sonora delle schede audio moderne.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbpro2.mdi]

;
;Selected by default if BLASTER variable is of type T6 or >, and AUTOEXEC does
;not contain AWEUTIL string
;
;Default I/O parms from BLASTER (A only)
;

.E BLASTER
.T3
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.NA AWEUTIL
.IOB
.IOA

.NAME
Creative Labs Sound Blaster(TM) 16

.SPECIAL_TEXT
Questo driver Š stato progettato per le Sound Blaster 16 che non sono dotate 
della scheda add-on General MIDI o Wave Blaster.

Comunque l'AWE-32 pu• funzionare anche col driver Sound Blaster 16, i 
possessori dell'AWE-32 possono selezionare il driver "Creative Labs 
AWE-32(TM) General MIDI" per ottimizzare la qualit… del suono.  
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbpro2.mdi]

;
;Selected by default if BLASTER variable is of type T2, T4, or T5,
;no other "clone" variable exists, and inp(388) == 0x00
;
;Default I/O parms from BLASTER (A only)
;

.E BLASTER
.T2
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOA

.SPECIAL_TEXT
Se la tua Sound Blaster Pro Š dotata del sintetizzatore Yamaha OPL-3, o se
l'audio non Š riprodotto correttamente con l'altro driver Sound Blaster Pro, 
devi selezionare questa opzione.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbpro1.mdi]

;
;Selected by default if BLASTER variable is of type T2, T4, or T5,
;no other "clone" variable exists, and inp(388) == 0x06
;
;Default I/O parms from BLASTER (A only)
;

.E BLASTER
.T2
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOA

.SPECIAL_TEXT
Gli utenti delle ultime versioni della Sound Blaster Pro possono 
utilizzare 18 voci e 2 operatori FM stereo selezionando questo driver.
Comunque, molte schede Sound Blaster Pro e compatibili, incluso la 
Sound Blaster 16, utilizzano il chipset OPL-3, pi— potente. Con queste
schede aggiornate, puoi selezionare il driver "Creative Labs Sound 
Blaster(TM) 16".
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[pas.mdi]

;
;Selected by default if MVSOUND exists in CONFIG.SYS, and inp(388) == 0x06
;
;No configuration allowed
;

.C MVSOUND.SYS
.ION

.SPECIAL_TEXT
Solo i possessori delle ultime versioni della Pro Audio Spectrum Media 
Vision possono selezionare questo driver. L'utility Media Vision 
MVSOUND.SYS deve essere caricata in memoria, o la tua scheda non sar… 
rilevata.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[pasplus.mdi]

;
;Selected by default if MVSOUND exists in CONFIG.SYS, and inp(388) == 0x00
;
;No configuration allowed
;

.C MVSOUND.SYS
.ION

.SPECIAL_TEXT
I possessori delle schede Media Vision Pro Audio Spectrum Plus e Pro 
Audio Spectrum 16 possono selezionare questo driver. L'utility Media
Vision MVSOUND.SYS deve essere caricata in memoria, o la tua scheda non
sar… rilevata.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[adlibg.mdi]

;
;Selected by default if GOLD variable exists in AUTOEXEC.BAT
;
;Default I/O parms from driver  
;

.E GOLD
.IOD

.SPECIAL_TEXT
Questo driver supporta la scheda AdLib Gold Music Synthesizer in modalit…
4 operatori FM.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[adlib.mdi]

;
;Never selected by default
;
;No configuration -- always at $388
;

.ND
.ION

.SPECIAL_TEXT
Questo driver pu• essere utilizzato con una scheda compatibile AdLib
FM music synthesizer che non ha bisogno di TSR software per la 
compatibilit… FM AdLib. Gli utilizzatori di schede General MIDI pi—
sofisticate possono selezionare il driver AdLib solo se si verificano
problemi con il driver General MIDI, siccome il vecchio chipset AdLib 
OPL-2 non permette una migliore qualit… audio, che Š invece disponibile
con le moderne schede.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[opl3.mdi]

;
;Never selected by default
;
;No configuration -- always at $388
;

.ND
.ION

.NAME
ESS Technology ES688 FM Audio

.SPECIAL_TEXT
Questo driver supporta i sistemi equipaggiati con la tecnologia ESS 
e chipset ES688.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[esfm.mdi]

;
;Never selected by default
;
;Configuration from driver
;

.ND
.IOD

.NAME
ESS Technology ES1688, ES1788, ES1888 Enhanced FM Audio

.SPECIAL_TEXT
Questo driver supporta sistemi equipaggiati con la tecnologia ESS e chipset
ES1688, ES1788, o ES1888. Un'audio FM avanzato Š disponibilile con questo
driver. Se si verificano dei problemi, seleziona il driver 'Tecnologia ESS 
ES688 Audio FM'.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[opl3.mdi]

;
;Never selected by default
;
;No configuration -- always at $388
;

.ND
.ION

.SPECIAL_TEXT
Questo driver serve per le schede basate sul sintetizzatore FM Yamaha OPL-3,
incluso quelle non supportate da nessun'altro driver della lista.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[mt32mpu.mdi]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.SPECIAL_TEXT
Anche se la Roland MT-32 non Š General MIDI compatibile, utilizza 
l'interfaccia hardware standard MPU-401 per comunicare con le applicazioni. 
I proprietari della MT-32 che usano controller Adaptec SCSI possono 
selezionare nel men— successivo "Configurazione manuale" per ridurre i 
problemi di rilevamento sulla MPU-401.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[tandy.mdi]

;
;Never selected by default
;
;No configuration allowed
;

.ND
.ION

.SPECIAL_TEXT
Questo driver supporta la Tandy 1000 a 3 voci e compatibili.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[pcspkr.mdi]

;
;Never selected by default
;
;No configuration allowed
;

.ND
.ION

.SPECIAL_TEXT
Questo driver supporta lo speaker interno del PC (1 voce), ma offre 
ovviamente un suono di bassa qualit….
.END_SPECIAL_TEXT

