Windows 3.1 256 Color Display Driver Release Notes
Copyright 1993 Microsoft Corporation
--------------------------------------------------
This disk contains a new high-speed 256 color display driver
for Windows 3.1 which supports most non-accelerated Super VGA 
display types.  If you have a Video card other than what is 
listed below you may not want to use these drivers.

For 800x600 256 colors and 1024x768 256 colorsresolutions 
you will need 1Mb of memory on you video card.    

You can install this driver by using Windows 
Setup to select one of the following display types:

	Super VGA  640x480 256 colors
	Super VGA  800x600 256 Large    ; Large fonts
	Super VGA  800x600 256 Small    ; Small fonts
	Super VGA 1024x768 256 Large    ; Large fonts
	Super VGA 1024x768 256 Small    ; Small fonts

Displays supported by these selections include the following:

	ATI VGA series, including
		ATI VGA Wonder
		ATI VGA Wonder Plus
		ATI VGA Wonder 24XL

	Cirrus Logic VGA (6420, 5420 series)

	Oak Technology VGA (077 series)

	Paradise VGA, including
		Paradise VGA 1024
		Paradise VGA Professional

	Trident VGA (8900C series) *, including
		Trident Impact

	Tseng VGA (ET4000 series) **, including:
		Boca VGA
		Cardinal VGA
		Diamond Speedstar series
		Everex Viewpoint series
		Metheus Premier VGA
		Orchid Prodesigner II
		Sigma VGA Legend
		STB Powergraph

	Video Seven VGA, including
		Video Seven FastWrite
		Video Seven 1024i
		Video Seven VRAM
		Video Seven VRAM II

	Western Digital VGA


*  NOTE:  MS-DOS applications run on Trident adapters may not
          be restored correctly when switched back to full-screen
          mode from Windows.

** NOTE:  MS-DOS applications run on some Tseng ET4000 adapters
	  may not be restored correctly when switched back to
          full-screen mode from Windows.  If this happens,
          use Windows Setup to select one of the ET4000 options.
          However, this may slow the operation of windowed
          MS-DOS applications.
       


