REM                    FLCS/TQS PROGRAMMING TEMPLATE
REM
REM B50 FILENAME: QWerewolf__  DESCRIPTION: TQS file for Werewolf VS. Comanche
REM
REM WRITTEN BY: Thrustmaster_____________________________  DATE: ___________
REM
REM NAME OF GAME AND PUBLISHER: werewolf by NovaLogic_______________________
REM ________________________________________________________________________
REM
REM
    USE TQS
REM
REM
    RATE 50
REM
REM ***********************MACRO DEFINITION FILE***************************
REM
    MDEF werewolf
REM
REM
REM ****************************FLCS SETTINGS******************************
REM
REM FIRST TRIGGER CLICK
REM
rem BTN TG1
REM
REM SECOND TRIGGER CLICK
REM
rem  BTN TG2
REM
REM BUTTONS S1 THRU S4 (S1=INDEX FINGER, S2=THUMB, S3=PINKY, AND
REM S4=PADDLE SWITCH ON FLCS).
REM
    BTN S1 AutoHover
    BTN S2 TargetSelect
    BTN S3 Chaff
    BTN S4 Flares
REM
REM HAT SWITCHES H1 THRU H4.  EACH HAT SWITCH FUNCTIONS AS A 5-WAY SWITCH,
REM THE POSITIONS CORRESPONDING TO THE 4 BASIC DIRECTIONS, AND THE MIDDLE
REM POSITION.
REM
REM H1=LARGE HAT AT TOP OF FLCS
    BTN H1U CockpitView
    BTN H1D LookBack
    BTN H1L LookLeft
    BTN H1R LookRight
    BTN H1M
REM
REM H2=SMALL HAT BELOW BUTTON S2
    BTN H2U MapZoomIn
    BTN H2D MapZoomOut
    BTN H2L TAS
    BTN H2R Map
    BTN H2M
REM
REM H3=SECOND LARGER HAT BELOW H1
    BTN H3U LeftTAC+
    BTN H3D TAS
    BTN H3L Stats
    BTN H3R Damage
    BTN H3M
REM
REM H4=HAT ON LEFT SIDE OF FLCS
    BTN H4U TailRotorLeft
    BTN H4D TailRotorRight
    BTN H4L AutoHover
    BTN H4R AutoHover
    BTN H4M
REM
REM ****************************WCS SETTINGS*******************************
REM
REM BUTTONS T1 THRU T10 ARE USED BY THE TQS.
    BTN T1 TargetSelect
    BTN T2 Panoramic
    BTN T3 ChaseCam
    BTN T4 DropCam
    BTN T5 PrevDropCam
    BTN T6 Cannon
    BTN T7 vikers
    BTN T8 archers
    BTN T9 Artillery
    BTN T10 Wingman
REM BUTTONS T11-T14 CORRESPOND TO THE FOUR MOUSE DIRECTIONS, AND WILL
REM GENERATE A REPEATING CHARACTER AS LONG AS THE TRACK BALL IS BEING
REM ROLLED.  BUTTONS T11-T14 ARE DESIGNED FOR USE IN SIMS THAT DON'T
REM SUPPORT THE MOUSE DIRECTLY.  IF YOUR SIM INCLUDES MOUSE SUPPORT, THEN
REM YOU SHOULD OMIT BUTTONS T11-T14.
rem BTN T11
rem BTN T12
rem BTN T13
rem BTN T14
REM
REM THROTTLE COMMANDS.  NOTE: OMIT THE 'THR' STATEMENT TO USE THE THROTTLE AS
REM AN ANALOG DEVICE.
REM
rem THR
REM
REM USE THE MINIMUM THROTTLE BUTTON SETTING TO CONTROL THE THROTTLE WHEN
REM PULLED FULLY BACK.
REM
rem BTN MT
REM
REM ***********************************************************************

RNG 1 3 MapZoomIn MapZoomOut
ANT 2 5 vikers archers Cannon FireTwoRockets Artillery
